Test tables

## Message Header Format

The following is the BGP version 4 message header format:

|  |  |  |  |
| --- | --- | --- | --- |
| **bit offset** | **0–15** | **16–23** | **24–31** |
| **0** | Marker | | |
| **32** |
| **64** |
| **96** |
| **128** | Length | Type |  |

* **Marker**: Included for compatibility, must be set to all ones.
* **Length**: Total length of the message in [octets](https://en.wikipedia.org/wiki/Octet_(computing)), including the header.
* **Type**: Type of BGP message. The following values are defined:
  + Open (1)
  + Update (2)
  + Notification (3)
  + KeepAlive (4)
  + Route-Refresh (5)