* 1. Refuse all incoming BGP connections.
  2. Start the initialization of event triggers.
  3. Initiates a TCP connection with its configured BGP peer.
  4. Listens for a TCP connection from its peer.
  5. Changes its state to Connect.